**Requirements:**

|  |  |
| --- | --- |
| **Components** | **Quantity** |
| Arduino Uno (Atmega 328p) | 1 |
| Potentiometer | 2 |
| Tactile switches | 6 |
| LCD display | 1 |
| Buzzer | 1 |
| Relays | 1 to 4 |
| Pump | 1 to 4 |

If you want, you can replace the pumps with lights. Therefore, we are using 1 to 4 relays in order to customize the number of pumps needed as per the user.